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CPU 110 datasheet
LADV100 basic controller. Order number LV100-C110-14DDT.
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Wartens LADV controllers are virtual PLCs that run in a web browser, for learning, for testing logic and for preparing for commissioning. They are not real time, not safety rated, and they cannot control equipment.
Overview
Small fixed-I/O controllers for learning ladder logic. Enough inputs and outputs for a motor station, a set of traffic lights or a garage door, and small enough that every channel is in view.
8 digital in, 6 digital out. The first controller.
Technical data
	Property
	Value

	Series
	LADV100 Basic

	CPU
	CPU 110

	Order number
	LV100-C110-14DDT

	Variant, as printed
	DC/DC/DC

	Digital inputs
	8

	Digital outputs
	6

	Analog inputs
	0

	Analog outputs
	0

	Expansion slots
	None, fixed I/O

	Program memory, ladder
	64 tags, 32 rungs, 2 routines

	Program memory, Structured Text
	64 variables, 256 statements, 4 program organisation units

	Fastest scan
	20 ms

	Watchdog
	150 ms per scan

	Retentive memory
	No. Every start is a cold start

	Languages
	Ladder (LADX), IEC 61131-3 Structured Text

	Tasks
	Cyclic and event tasks, priorities from 0, non-preemptive

	Online functions
	Watch, modify, force I/O, 64-entry diagnostic buffer

	Status lamps
	RUN, STOP, ERROR, MAINT

	Firmware
	V1.0.0

	Serial number, as printed
	WL26-110-71090

	Availability
	Available in the VPLC lab



Addressing
Structured Text names a channel by its IEC 61131-3 direct address. Ladder wires tags to channels in the order the tags are listed.
	Channels
	Count
	Structured Text addresses

	Digital inputs
	8
	%IX0.0 to %IX0.7

	Digital outputs
	6
	%QX0.0 to %QX0.5

	Analog inputs
	0
	none

	Analog outputs
	0
	none



Status lamps
	Lamp
	Colour
	Meaning

	RUN
	Green
	The program is executing and outputs are live.

	STOP
	Amber
	Stopped. Outputs are off.

	ERROR
	Red
	Faulted. Outputs are off until the fault is reset. The diagnostic buffer gives the code.

	MAINT
	Amber
	At least one I/O point is forced.



Not included
1. No fieldbus, no network protocols and no physical I/O.
1. No hard real-time guarantee: scans run on simulated time in the browser.
1. No safety rating. Safety functions belong in a safety-rated controller.
Related documents
1. LADV system manual, LADV-SM
1. Structured Text programming manual, LADV-PM-ST
1. Ladder instruction reference, LADV-IR-LD
1. Diagnostic and fault codes, LADV-DC
