Wartens
info@wartens.com  ·  ladx.ai

LADV300 I/O modules datasheet
Expansion modules for the LADV300 modular controllers.
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Wartens LADV controllers are virtual PLCs that run in a web browser, for learning, for testing logic and for preparing for commissioning. They are not real time, not safety rated, and they cannot control equipment.
Modules
	Module
	Order number
	Channels
	Rating, as printed
	Description

	LADV-DI16
	LV300-DI16D
	16 DI
	24 V DC
	16 digital inputs, 24 V DC sinking

	LADV-DO16
	LV300-DO16T
	16 DO
	24 V DC 0.5 A
	16 digital outputs, 24 V DC sourcing

	LADV-AI8
	LV300-AI8U
	8 AI
	U / I
	8 analog inputs, 0 to 10 V or 4 to 20 mA

	LADV-AO4
	LV300-AO4U
	4 AO
	U / I
	4 analog outputs, 0 to 10 V or 4 to 20 mA



Configuration
1. Modules fit the LADV300 CPUs only: CPU 310 with 8 slots, CPU 350 with 16 slots.
1. Channels add to the CPU's own, in slot order. The download checks the program's I/O against the total and names the shortfall.
1. Analog channels read and write INT, 0 to 1000 for 0 to 100 percent of span, the same as the CPU's own analog channels.
1. The power module, LADV-PS24, is drawn on the rack and needs no configuration.
